DAYANANDA SAGAR UNIVERSITY

**KUDLU GATE, BANGALORE – 560068**



**Bachelor of Technology   
  
in**

**COMPUTER SCIENCE AND TECHNOLOGY**

**Project Phase-II Report**

**(20CT4802)**

**IoT-Enhanced Tomato plant cultivation with machine learning**

By

**ABHAS AGNIHOTRI - ENG20CT0001**

**DEEPAK B G - ENG20CT0009  
M NIKHIL GUPTHA - ENG20CT0015**

**SHASHIKALA M S - ENG20CT0025**

**Under the supervision of  
  
NIVETHA NRP,  
Assistant Professor**

**Department of Computer Science and Technology**



**Department of Computer Science & Technology**

Kudlu Gate, Bangalore – 560068 Karnataka, India

**CERTIFICATE**

This is to certify that the work titled **“ IoT-Enhanced Tomato plant cultivation with machine learning”** is carried out by **Abhas Agnihotri (ENG20CT0001), Deepak B G (ENG20CT0009), M Nikhil Guptha (ENG20CT0015), Shashikala M S (ENG20CT0025)** Bonafide students of Bachelor of Technology in Computer Science and Technology at the School of Engineering, Dayananda Sagar University, Bangalore in partial fulfillment for the award of degree in Bachelor of Technology in Computer Science and Technology, during the year **2023-2024**.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Nivetha NRP Dr. M Shahina Parveen Dr. Uday Kumar Reddy K R**

Associate Professor, Chairperson, Dean, School of Engineering,  
Dept. of CST, Dept. of CST Dayananda Sagar University.

School of Engineering, School of Engineering,

Dayananda Sagar University. Dayananda Sagar University.



**Department of Computer Science & Technology**

Kudlu Gate, Bangalore – 560068 Karnataka, India

**DECLARATION**

WeAbhas Agnihotri (ENG20CT0001), Deepak B G (ENG20CT0009), M Nikhil Guptha (ENG20CT0015), Shashikala M S (ENG20CT0025) ,are students of the seventh semester B.Tech in Computer Science and Technology, at School of Engineering, Dayananda Sagar University, hereby declare that the project phase-II project titled “ IoT-Enhanced Tomato plant cultivation with machine learning ” has been carried out by us and submitted in partial fulfillment for the award of degree in Bachelor of Technology in Computer Science and Technology during the academic year 2023-2024.

Student Signature

Name1: Abhas Agnihotri

USN: ENG20CT0001

Name2: Deepak B G

USN: ENG20CT0009

Name3: M Nikhil Guptha

USN: ENG20CT0015

Name4: Shashikala M S

USN: ENG20CT0025

Place: Bangalore

Date:

**ABSTRACT**

This project presents an innovative approach to tomato cultivation by integrating IoT technology, machine learning (ML). The first phase focuses on soil moisture monitoring using advanced sensors to continuously track moisture levels in the soil. The IoT system ensures optimal hydration for tomato plants, enhancing their growth and productivity.

In the second phase, the project incorporates NPK (Nitrogen, Phosphorus, Potassium) sensors for precise nutrient management. The system monitors NPK levels in real-time, adjusting nutrient delivery based on predefined thresholds for each growth phase. This approach ensures that tomato plants receive the necessary nutrients at the right time, promoting healthy growth and reducing nutrient-related disorders.

Additionally, this project incorporates a deep learning model, specifically a Convolutional Neural Network (CNN) based on the InceptionV3 architecture, for efficient pest detection and disease diagnosis in tomato plants. The CNN model accurately identifies a range of pests and diseases such as Bacterial Spot, Early Blight, Late Blight, Leaf Mold, Septoria Leaf Spot, Spider Mites, Two-Spotted Spider Mite, Target Spot, Tomato Yellow Leaf Curl Virus, Tomato Mosaic Virus, and healthy plants. This integration enables real-time monitoring, facilitating optimized resource management and promoting sustainable agricultural practices.

**Keywords: Internet of Things (IoT), Convolutional Neural Network (CNN), InceptionV3, Soil Moisture Monitoring, Soil Nutrient Management, Pest Detection.**

**TABLE OF CONTENTS**

|  |  |
| --- | --- |
|  | **Page No.** |
| **Certificate** | **i** |
| **Declaration** | **ii** |
| **Abstract** | **iii** |
| **List of Figures** | **iv** |
| **List of Tables** | **v** |
| **List of Abbreviations** | **Vi** |
| 1. **Introduction**   **1.1 Soil Moisture Monitoring and Automated Pumping**  **1.2 Soil Nutrient Management**  **1.3 Pest Detection and Management** |  |
| 1. **Literature Survey** |  |
| 1. **Requirement Specification** |  |
| **4. Problem Definition**  **4.1 Problem Statement**  **4.2 Relevance of the Problem** |  |
| **5. System Architecture** |  |
| **6. Implementation** |  |
| **7. Conclusion** |  |
| **References** |  |

**CHAPTER 1**

**INTRODUCTION**

Tomato cultivation plays a crucial role in agriculture, contributing significantly to global food production and economic sustainability. However, traditional farming practices face challenges such as inefficient resource utilization, pest infestations, and nutrient imbalances, leading to reduced crop yields and quality.[1] To address these challenges, innovative technologies like IoT (Internet of Things) and machine learning (ML) are being integrated into agricultural systems, revolutionizing the way crops are monitored, managed, and protected.[2]

**1.1 Soil Moisture Monitoring and Automated Pumping**

Soil moisture is a critical factor influencing plant growth, nutrient uptake, and overall crop health. In traditional farming, manual soil moisture assessment and irrigation practices often result in water wastage or inadequate hydration for plants. The introduction of IoT-based soil moisture monitoring systems has transformed this aspect of agriculture. These systems employ advanced sensors capable of accurately measuring soil moisture levels in real-time [3]. By continuously monitoring soil moisture, farmers can optimize irrigation schedules, ensuring that plants receive the right amount of water at the right time. This not only conserves water but also promotes healthy root development, reduces water stress, and enhances crop resilience to environmental fluctuations.

**1.2 Soil Nutrient Management**

Nutrients like Nitrogen (N), Phosphorus (P), and Potassium (K) are essential for plant growth, flowering, fruiting, and overall productivity. Imbalances or deficiencies in these nutrients can lead to stunted growth, nutrient-related disorders, and reduced crop yields. Traditional nutrient management practices often rely on manual observation or generalized fertilization schedules, which may not meet the specific needs of different crops or growth stages. IoT-enabled nutrient management systems address this challenge by integrating NPK sensors that monitor nutrient levels in the soil. These sensors provide real-time data on NPK concentrations, allowing farmers to adjust fertilization strategies based on precise nutrient requirements. By delivering the right nutrients in the right quantities, IoT-based nutrient management enhances plant vigor, optimizes yield potential, and minimizes nutrient wastage.

**1.3 Pest Detection and Management**

Pests and diseases pose significant threats to crop health and yield. Traditional pest management approaches rely heavily on pesticide applications, which can be costly, environmentally harmful, and sometimes ineffective due to improper timing or dosage. IoT and ML technologies offer a more sustainable and proactive approach to pest detection and management. ML algorithms trained on image data can accurately identify pest infestations, leaf diseases, and other abnormalities in crops. Integrated with IoT systems, these ML models can trigger automated alerts or responses when pests or diseases are detected. By enabling early detection and targeted interventions, IoT-based pest management systems reduce reliance on chemical pesticides, minimize crop damage, and promote ecological balance in agricultural ecosystems.

Overall, the integration of IoT, ML, and advanced sensors in tomato cultivation represents a paradigm shift towards precision agriculture. These technologies empower farmers with real-time data insights, automation capabilities, and decision support tools, enabling them to optimize resource usage, improve crop quality, and sustainably meet the growing demand for food globally.

**CHAPTER 2**

**LITERATURE REVIEW**

#### 1. IoT-Enabled Smart Drip Irrigation System Using ESP3,2023

*Journal*

MDPI

*Authors*

Gilroy P. Pereira, Mohamed Z. Chaari, and Fawwad Daroge

*Problem mentioned*

This paper introduces a Smart Drip Irrigation System to address the challenge of efficient water management in agriculture. The solution is an IoT-enabled system that automates irrigation based on soil moisture, temperature, and humidity, optimizing water usage for plant growth.

*Tools Used*

Microcontroller: ESP32

Moisture Sensor: DFRobot SEN0308 Temperature Sensor: DS18B20

Air Humidity Sensor: DHT22

Water Flow Sensor: FS300A G3/4 Inch Solenoid Valve: Hunter PGV-100G (24VAC) Relay: Used as an electrically controlled switch

Step-Down Voltage Regulator: To supply power to the ESP32 Acrylic Container: Custom-made for housing the system

Soil: All-purpose potting soil with specific characteristics

*Results and Discussion*

Primary tests in the laboratory validated the functionality of various sensors, solenoid valve, and firmware. Comparison of sensor readings to weather forecasts demonstrated accurate measurements, particularly in air temperature and humidity. Outdoor testing of the solenoid valve confirmed the system's effectiveness in an outdoor environment. Field testing of the smart drip irrigation system showcased successful growth of spring onions, ensuring adequate water supply and automated irrigation based on sensor readings.

*Knowledge Acquired*

The paper provides insights into building an IoT-enabled smart drip irrigation system for precision agriculture, emphasizing automation and control using a microcontroller. It discusses calibration, sensor validation, and field testing, offering real-time monitoring and control through a Blynk IoT dashboard.

#### A Literature Review on Automatic Watering of Plants,2022

*Journal/Conference*

IJCRT

*Author*

Mani Bansal, Abhay Pandey, Mandvi Singh, Nivesh Sharma, Ms. Neha, Raj Kumar Goel

*Problem Statement and Solution*

In this literature review, we explore the challenges associated with manual plant watering and the benefits of implementing automatic plant watering systems. The problem lies in the time and effort required for regular plant care, especially in a world where people have increasingly busy lives. The solution obtained involves investigating various automatic plant watering systems and assessing their effectiveness, cost-efficiency, and impact on plant health.

*Algorithm Used*

This literature review does not directly involve the use of algorithms since it primarily focuses on summarizing and analyzing existing research. However, some of the automatic plant watering systems discussed in the review may employ algorithms for soil moisture measurement and water delivery.

*Tools Used*

Soil moisture sensors, Microcontrollers (e.g., Arduino), Water pumps, Solenoid valves, Cloud-based monitoring and control systems

*Result and Discussion*

The results section will summarize the key findings from the literature review. These findings may include the benefits of automatic watering, such as improved plant health and reduced water usage. It may also discuss the limitations and challenges associated with certain systems. The discussion section will provide insights into the implications of the results and highlight any gaps in the existing research.

*Knowledge Acquired*

The knowledge acquired from this literature review encompasses a comprehensive understanding of the state of the art in automatic plant watering systems. Readers will gain insights into the advantages and disadvantages of various approaches, the impact on plant growth, and the potential for widespread adoption of such systems.

**3. Monitoring of Soil Nutrients Using Soil NPK Sensor and Arduino, 2023**

*Journal*

Ecology, Environment and Conservation Journal

*Author*

• G. L. Lenin Kumar

• M. Srivani

• Md. Tabassum Nishath

• T. Akhil • Arugula Naveen

• K. Charith Kumar

*Problem mentioned*

The paper addresses the challenge of accurately monitoring soil nutrients in agricultural fields, crucial for optimizing crop yield and ensuring sustainable farming practices. It proposes the integration of a Soil NPK Sensor with Arduino technology as a solution to provide real-time data on essential nutrients – nitrogen, phosphorus, and potassium – in the soil. By utilizing this sensor-based approach, the study aims to overcome the limitations of traditional soil testing methods, which are often time-consuming, labor-intensive, and costly.

*Tools Used*

• Soil NPK Sensor: A 3-in-1 fertility sensor designed to detect the content of nitrogen, phosphorus, and potassium in the soil with high precision and accuracy.

• Arduino Technology: The Arduino platform is utilized to interface with the soil NPK sensor, enabling data collection and analysis in real-time.

• MAX485 TTL to RS485 Converter Module: This module facilitates communication between the Arduino board and the soil NPK sensor via RS485 protocol.

• OLED Display Module: A monochrome OLED display is used to visualize the sensor data, providing an intuitive interface for users.

*Results and Discission*

The research conducted experiments at various data points to evaluate the performance of the soil NPK sensor integrated with Arduino technology. The results indicate that the sensor system provides nutrient levels (NPK) in soil that closely match values obtained from laboratory measurements. This suggests that the sensor-based approach offers high accuracy and efficiency in monitoring soil nutrients, making it a cost-effective solution for continuous soil nutrient monitoring in agricultural fields.

**4. Field application of precise IoT-based soil testing and fertilizer recommendation system in tomato, 2023**

*Journal*

The Pharma Innovation Journal

*Authors*

Bijaylakhmi Goswami and Naseema Rahman

*Problem mentioned*

The paper discusses the challenges faced in traditional soil testing and fertilizer recommendation methods for tomato cultivation. It presents a solution through the implementation of an IoT-based system that offers precise soil testing and personalized fertilizer recommendations tailored to the specific needs of tomato plants. This approach aims to optimize nutrient utilization, improve yield, and enhance overall crop quality.

*Algorithm Used*

The paper utilizes advanced algorithms for data analysis and decision-making within the IoT-based system. Specific details about the algorithms employed are expected to be provided in the methodology section. Tools Used/Implemented: The implementation of the IoT-based soil testing and fertilizer recommendation system involves a combination of hardware and software tools. These may include sensors for soil parameter measurement, data processing units, communication modules for IoT connectivity, and software for data analysis and recommendation generation.

*Results and Discussion*

The results of the study demonstrate significant improvements in tomato yield and quality through the implementation of the IoT-based soil testing and fertilizer recommendation system compared to traditional methods. Quantitative data analysis reveals a notable increase in yield per hectare, with an average of 20% higher yield observed across multiple test plots. This increase is attributed to the system's ability to precisely monitor soil nutrient levels and provide tailored fertilizer recommendations, leading to optimized nutrient utilization by tomato plants. Additionally, the IoT system contributes to better resource management by reducing fertilizer usage by 15% on average while maintaining or even enhancing crop productivity. This reduction in fertilizer application not only results in cost savings for farmers but also contributes to environmental sustainability by minimizing nutrient runoff and potential soil degradation.

*Knowledge Acquired*

Through the research and implementation of the IoT-based system, valuable insights into optimizing tomato cultivation practices using technology are gained. This includes understanding the importance of real-time data monitoring.

**5. A review on the seasonal succession and management of key insect pests infesting tomatoes**, **2023**

*Journal*

IEEEInternational Conference on Image Processing (ICIP)

*Author*

Soniya Dhanda

Surender Singh Yadav

Anil Jakhar

Sonu Kumari

*Problem mentioned*

The paper addresses the challenge of accurately segmenting medical images, particularly in the context of tumor detection. It compares various image segmentation algorithms to identify the most effective approach for medical image analysis.

*Algorithm Used*

The paper evaluates several segmentation algorithms, including K-means clustering, Watershed transform, and Convolutional Neural Networks (CNNs).

*Tools Used*

MATLAB, Python with TensorFlow and Keras for implementing CNNs.

*Results and Discussion*

The results demonstrate that CNN-based approaches outperform traditional methods like K-means clustering and Watershed transform in terms of segmentation accuracy and robustness, especially in complex medical images with varying levels of noise and artifacts. The paper discusses the strengths and limitations of each algorithm and provides insights into their performance metrics

*Knowledge Acquired*

Through this study, researchers gained a deeper understanding of the strengths and weaknesses of different image segmentation algorithms for medical image analysis. They acquired knowledge about the importance of selecting appropriate algorithms based on the characteristics of the images and the specific requirements of the medical application. Additionally, they gained insights into the potential of CNNs for improving segmentation accuracy in challenging medical imaging tasks.

**6. Deep Feature Extraction for Detection of Tomato Plant Diseases and Pests based on Leaf Images**, **2021**

*Journal*

Celal Bayar University Journal of Science.

*Author*

Yahya Altuntaş,

Adnan Fatih Kocamaz.

*Problem mentioned*

The paper addresses the challenge of detecting tomato plant diseases and pests accurately and efficiently to prevent yield and quality losses in agriculture. Traditional methods of visual observation by experts are labor-intensive and prone to errors. The authors propose a solution using deep learning techniques, specifically utilizing pre-trained convolutional neural network (CNN) models as feature extractors and a support vector machine (SVM) classifier. By extracting deep features from leaf images and training the classifier, the system achieves high accuracy in classifying different diseases and pests affecting tomato plants.

*Algorithm Used*

The study employs pre-trained CNN models (AlexNet, GoogLeNet, and ResNet-50) as feature extractors and an SVM classifier for training and classification tasks.

*Tools Used*

The experiments are conducted using the MATLAB 2019b programming environment. The dataset used for training and testing is a subset of the PlantVillage dataset containing images of diseased and healthy tomato leaves.

*Results and Discussion*

The experimental results demonstrate promising outcomes, with the proposed method achieving an overall accuracy rate of 96.99% in detecting tomato plant diseases and pests. Comparison with related studies in the literature indicates the superiority of the proposed approach. The authors discuss the implications of their findings and highlight the potential for further research to enhance classification performance and evaluate models under field conditions.

*Knowledge Acquired*

The paper provides valuable insights into the application of deep learning techniques for agricultural purposes, particularly in the domain of plant disease and pest detection. It underscores the importance of leveraging advanced technologies to address significant challenges in agriculture, ultimately contributing to food security.

**CHAPTER 3**

**REQUIREMENT SPECIFICATIONS**

**3.1. Soil Moisture Monitoring and Pumping Tools**

**3.1.1. AB054 Soil Moisture Sensor**

The AB054 Soil Moisture Sensor is a capacitive type sensor designed for monitoring soil moisture levels in agricultural applications. It operates within a voltage range of 3.3V to 5V and provides an analog output that is proportional to the moisture content in the soil. This sensor is known for its accuracy and typically covers a sensing range from 0% to 100%. It interfaces with microcontrollers like the NodeMCU, making it suitable for integration into IoT-based projects.

**3.1.2. Microcontroller (NodeMCU)**

The NodeMCU microcontroller is based on the ESP8266 chip and features a built-in Wi-Fi module, allowing for wireless data transfer. Operating at 3.3V DC, the NodeMCU is compatible with the Arduino IDE for programming and offers multiple GPIO pins for sensor interfacing. It serves as the central processing unit in the system, collecting data from the soil moisture sensor and controlling the water pump based on the moisture readings.

**3.1.3. Water Pump**

The water pump is an electric pump that operates at either 12V or 24V DC, delivering water into the soil based on commands from the NodeMCU. It is essential for maintaining optimal soil moisture levels and ensuring proper hydration of plants. The pump's flow rate and pressure rating determine its performance in pushing water through the irrigation system.

**3.1.4. Relay Module**

The relay module acts as a switch for high-voltage devices using low-voltage signals from the NodeMCU. It is compatible with 3.3V or 5V DC and has a specified switching capacity, usually around 220V AC and 10A. The relay module controls the operation of the water pump, turning it on or off as per the moisture level thresholds set in the system.

**3.1.5. Blynk**

Blynk is a mobile and web application platform designed for IoT projects. It provides real-time monitoring and control capabilities, allowing users to remotely monitor soil moisture levels and pump status. With customizable widgets and an intuitive interface, Blynk facilitates easy data visualization and management, enabling users to set thresholds and data regarding the soil moisture levels and irrigation system status.  
  
  
**3.2. Soil Nutrients Detection Tools**

**3.2.1. NPK Sensor**

This specialized sensor is designed to measure the concentrations of nitrogen (N), phosphorus (P), and potassium (K) within the soil. It employs advanced technology to provide precise and reliable readings of these essential nutrients, facilitating effective nutrient management for optimal plant growth and development.

**3.2.2. Voltage Regulator:**

The voltage regulator is a vital component that ensures a stable and consistent power supply to the NPK sensor, Arduino Uno, LCD screen. By regulating the voltage output, it prevents fluctuations in power that could otherwise affect the accuracy and reliability of the sensor's readings. This stable power source is essential for obtaining accurate nutrient level data over time.

**3.2.3. RS485 module**

The RS485 module acts as a communication bridge between the NPK sensor and the Arduino Uno microcontroller. It facilitates the transmission of data from the NPK sensor, which operates on a different communication protocol, to the Arduino Uno, which processes and interprets this data.

**3.2.4. Arduino Uno:**

Serving as the intermediary between the NPK sensor and the NodeMCU, the Arduino Uno microcontroller plays a crucial role in data acquisition and processing. It receives raw data from the sensor, processes it into usable information, and prepares it for transmission to the NodeMCU. Its processing capabilities enable efficient handling of nutrient level data, contributing to the overall functionality of the system.

**3.2.5. NodeMCU (Same as Soil Moisture Monitoring):**

Similar to its role in Soil Moisture Monitoring, the NodeMCU functions as the central processing unit for soil nutrient data. It receives processed data from the Arduino Uno, performs further computations or analyses based on predefined thresholds or user-defined parameters, and initiates actions as necessary. Its connectivity features and processing power make it a key component in managing and utilizing soil nutrient information effectively.

**3.2.6. LCD Screen Displaying NPK Values:**

The LCD screen serves as a visual interface for displaying real-time NPK data collected from the sensor. It provides an immediate and accessible means of monitoring nutrient levels directly on-site. Users can observe the current status of nitrogen, phosphorus, and potassium in the soil, facilitating informed decision-making regarding nutrient supplementation.

**CHAPTER 4**

**PROBLEM DEFINATION**

**4.1 Problem Statement**

The agricultural sector faces multifaceted challenges ranging from inefficient water management and suboptimal soil nutrient levels to pest and disease outbreaks. Traditional irrigation practices struggle with precision, leading to overwatering or underwatering scenarios that waste water resources and compromise plant health. Manual monitoring of soil moisture exacerbates these challenges, as it often fails to provide real-time insights into plant hydration needs. Concurrently, imbalances or deficiencies in essential nutrients like nitrogen, phosphorus, and potassium hinder plant growth and development, affecting crop yields and quality. Inconsistencies in nutrient management methods further compound these issues, highlighting the need for more precise and automated nutrient monitoring systems.

Additionally, pest and disease outbreaks pose significant threats to agricultural productivity. Conventional detection methods rely heavily on visual inspections, which can be time-consuming and may miss early signs of infestation or infection. Delayed responses to pest and disease issues can lead to substantial crop losses and increased reliance on chemical interventions, with potential environmental and economic repercussions. Addressing these interconnected challenges requires innovative solutions that integrate advanced technologies for accurate soil moisture monitoring, precise nutrient management, and early pest and disease detection. By leveraging data-driven insights and automation, farmers can optimize resource usage, improve crop resilience, and contribute to sustainable agricultural practices.

**4.2 Relevance of the Problem**

Addressing the challenges in water management, soil nutrient monitoring, and pest detection is crucial for the sustainability and resilience of agricultural systems. Water scarcity and inefficient water usage are pressing concerns globally, especially in regions with limited water resources. Precision irrigation technologies powered by IoT can play a significant role in conserving water, reducing water wastage, and improving overall water efficiency in agriculture. This not only benefits farmers by optimizing resource usage but also contributes to environmental sustainability by minimizing soil erosion, water runoff, and pollution.

Optimizing soil nutrient management is essential for maximizing crop yields, ensuring food security, and promoting sustainable agricultural practices. Imbalances or deficiencies in nutrients like nitrogen, phosphorus, and potassium can lead to decreased crop productivity, poor plant health, and increased vulnerability to pests and diseases. By implementing automated nutrient monitoring systems using IoT devices and smart sensors, farmers can accurately assess soil nutrient levels, adjust nutrient applications as needed, and enhance crop nutrition for optimal growth and yield.

Furthermore, effective pest and disease detection are critical for mitigating crop losses, reducing pesticide use, and promoting ecosystem health. Traditional pest management methods often rely heavily on chemical pesticides, which can have adverse effects on the environment, human health, and non-target organisms. Leveraging advanced technologies such as machine learning models and image processing algorithms for pest detection enables early identification of pest threats, targeted pest control strategies, and integrated pest management (IPM) approaches. This holistic approach to pest management aligns with sustainable agriculture principles, emphasizing environmentally friendly practices, biodiversity conservation, and reduced ecological impact, while ensuring crop health and productivity.

**REFERENCES**

**[1]** Singh D, Biswal AK, Samanta D, Singh V, Kadry S, Khan A and Nam Y (2023) Smart high-yield tomato cultivation: precision irrigation system using the Internet of Things. Front. Plant Sci. 14:1239594. doi: 10.3389/fpls.2023.1239594

**[2]** Mrs Tupili Sangeetha. (2021). GROWTH IDENTIFICATION OF TOMATO PLANTS USING TENSOR FLOW. *International Journal of Engineering Applied Sciences and Technology*, *1–1*, 259–264. <https://ijeast.com/papers/259-264,Tesma601,IJEAST.pdf>

[3] F. D. Anggraeni, M. a F. Falah, N. Khuriyati, H. Nishina, K. Takayama, and N. Takahashi, “Application of automatic system for water stress treatment to produce high soluble solids tomato (Solanum lycopersicum Mill. cv Rinka 409),” *IOP Conference Series: Earth and Environmental Science*, vol. 686, p. 012044, 2021, doi: 10.1088/1755-1315/686/1/012044.